**Packet Tracer - Configuring Initial Switch Settings**

**Topology**

**Objectives**

**Part 1: Verify the Default Switch Configuration**

**Part 2: Configure a Basic Switch Configuration**

**Part 3: Configure a MOTD Banner**

**Part 4: Save Configuration Files to NVRAM**

**Part 5: Configure S2**

**Background**

In this activity, you will perform basic switch configurations. You will secure access to the command-line interface (CLI) and console ports using encrypted and plain text passwords. You will also learn how to configure messages for users logging into the switch. These banners are also used to warn unauthorized users that access is prohibited.

**Part 1:     Verify the Default Switch Configuration**

**Step 1:     Enter privileged EXEC mode.**

You can access all switch commands from privileged EXEC mode. However, because many of the privileged commands configure operating parameters, privileged access should be password-protected to prevent unauthorized use.

The privileged EXEC command set includes those commands contained in user EXEC mode, as well as the **configure**command through which access to the remaining command modes are gained.

a.     Click **S1** and then the **CLI** tab. Press Enter.

b.    Enter privileged EXEC mode by entering the **enable**command:

Switch> **enable**

Switch#

Notice that the prompt changed in the configuration to reflect privileged EXEC mode.

**Step 2:     Examine the current switch configuration.**

a.     Enter the **show running-config** command.

Switch# **show running-config**

**\*\* use space bar to print out 1 page of information \*\***

b.    Answer the following questions:

1)     How many FastEthernet interfaces does the switch have?

24

2)     How many Gigabit Ethernet interfaces does the switch have?

2

3)     What is the range of values shown for the vty lines?

llne vty 0 4

line vty 5 15

4)     Which command will display the current contents of non-volatile random-access memory (NVRAM)?

Switch#show running-config

5)     Why does the switch respond with startup-config is not present?

The switch responds with "startup-config is not present" because the start up configuration hasn't been saved yet.

**Part 2:     Create a Basic Switch Configuration**

**Step 1:     Assign a name to a switch.**

To configure parameters on a switch, you may be required to move between various configuration modes. Notice how the prompt changes as you navigate through the switch.

Switch# **configure terminal**

Switch(config)# **hostname S1**

S1(config)# **exit**

S1#

**Step 2:     Secure access to the console line.**

To secure access to the console line, access config-line mode and set the console password to **letmein**.

S1# **configure terminal**

Enter configuration commands, one per line. End with CNTL/Z.

S1(config)# **line console 0**

S1(config-line)# **password letmein**

S1(config-line)# **login**

S1(config-line)# **exit**

S1(config)# **exit**

%SYS-5-CONFIG\_I: Configured from console by console

S1#

Why is the **login** command required?

The login command is required because it makes it so the user will be prompted with a login request. without it, the user won't be able to access the router.

**Step 3:     Verify that console access is secured.**

Exit privileged mode to verify that the console port password is in effect.

S1# **exit**

Switch con0 is now available

Press RETURN to get started.

User Access Verification

Password:

S1>

**Note**: If the switch did not prompt you for a password, then you did not configure the **login** parameter in Step 2.

**Step 4:     Secure privileged mode access.**

Set the **enable** password to **c1$c0**. This password protects access to privileged mode.

**Note:**The **0** in **c1$c0** is a zero, not a capital O. This password will not grade as correct until after you encrypt it in Step 8.

S1> **enable**

S1# **configure terminal**

S1(config)# **enable password c1$c0**

S1(config)# **exit**

%SYS-5-CONFIG\_I: Configured from console by console

S1#

**Step 5:     Verify that privileged mode access is secure.**

a.     Enter the **exit**command again to log out of the switch.

b.    Press **<Enter>** and you will now be asked for a password:

User Access Verification

Password:

c.     The first password is the console password you configured for **line con 0**. Enter this password to return to user EXEC mode.

d.    Enter the command to access privileged mode.

e.     Enter the second password you configured to protect privileged EXEC mode.

f.     Verify your configurations by examining the contents of the running-configuration file:

S1# **show running-config**

Notice how the console and enable passwords are both in plain text. This could pose a security risk if someone is looking over your shoulder.

**Step 6:     Configure an encrypted password to secure access to privileged mode.**

The **enable password**should be replaced with the newer encrypted secret password using the **enable secret**command. Set the enable secret password to **itsasecret**.

S1# **config t**

S1(config)# **enable secret itsasecret**

S1(config)# **exit**

S1#

**Note**: The **enable secret** password overrides the **enable** password. If both are configured on the switch, you must enter the **enable secret** password to enter privileged EXEC mode.

**Step 7:     Verify that the enable secret password is added to the configuration file.**

a.     Enter the **show running-config**command again to verify the new **enable secret** password is configured.

**Note:**You can abbreviate **show running-config**as

S1# **show run**

b.    What is displayed for the **enable secret** password?

For the enable secret password, "5 $1$mERr$ILwq/b7kc.7X/ejA4Aosn0" is shown.

c.     Why is the **enable secret** password displayed differently from what we configured?

The enable secret password is displayed differently from what I configured because it is an automatically encrypted password.

**Step 8:     Encrypt the enable and console passwords.**

As you noticed in Step 7, the **enable secret** password was encrypted, but the **enable** and **console** passwords were still in plain text. We will now encrypt these plain text passwords using the **service password-encryption** command.

S1# **config t**

S1(config)# **service password-encryption**

S1(config)# **exit**

If you configure any more passwords on the switch, will they be displayed in the configuration file as plain text or in encrypted form? Explain.

If I configure any more passwords, they will be displayed as plain text. This is because I serviced the other passwords to be encrypted. If I wanted passwords to be re-encrypted, I would need to re-enter the "Switch(config)#service password-encryption" command.

**Part 3:     Configure a MOTD Banner**

**Step 1:     Configure a message of the day (MOTD) banner.**

The Cisco IOS command set includes a feature that allows you to configure messages that anyone logging onto the switch sees. These messages are called message of the day, or MOTD banners. Enclose the banner text in quotations or use a delimiter different from any character appearing in the MOTD string.

S1# **config t**

S1(config)# **banner motd "This is a secure system. Authorized Access Only!"**

S1(config)# **exit**

%SYS-5-CONFIG\_I: Configured from console by console

S1#

1)     When will this banner be displayed?

This banner will be displayed when the user first gets onto the router.

2)     Why should every switch have a MOTD banner?

Every switch should have a MOTD banner because It keeps users updated on various activities, and it can also be used to warn against un-authorized access.

**Part 4:     Save Configuration Files to NVRAM**

**Step 1:     Verify that the configuration is accurate using the show run command.**

**Step 2:     Save the configuration file.**

You have completed the basic configuration of the switch. Now back up the running configuration file to NVRAM to ensure that the changes made are not lost if the system is rebooted or loses power.

S1# **copy running-config startup-config**

Destination filename [startup-config]?**[Enter]**

Building configuration...

[OK]

What is the shortest, abbreviated version of the **copy running-config startup-config** command?

The shortest, abbreviated version of the copy running-config startup-config command is "copy run start".

**Step 3:     Examine the startup configuration file.**

Which command will display the contents of NVRAM?

The command that will display the contents of NVRAM is "Switch#show startup-configuration".

Are all the changes that were entered recorded in the file?

All the changes that are entered are recorded in the file.

**Part 5:     Configure S2**

You have completed the configuration on S1. You will now configure S2. If you cannot remember the commands, refer to Parts 1 to 4 for assistance.

**Configure S2 with the following parameters:**

a.     Name device: **S2**

b.    Protect access to the console using the **letmein** password.

c.     Configure an enable password of **c1$c0**and an enable secret password of **itsasecret**.

d.    Configure a message to those logging into the switch with the following message:

Authorized access only. Unauthorized access is prohibited and violators will be prosecuted to the full extent of the law.

e.     Encrypt all plain text passwords.

f.     Ensure that the configuration is correct.

g.    Save the configuration file to avoid loss if the switch is powered down.

**Suggested Scoring Rubric**

|  |  |  |  |
| --- | --- | --- | --- |
| **Activity Section** | **Question Location** | **Possible Points** | **Earned Points** |
| Part 1: Verify the Default Switch Configuration | Step 2b, q1 | 2 |  |
| Step 2b, q2 | 2 |  |
| Step 2b, q3 | 2 |  |
| Step 2b, q4 | 2 |  |
| Step 2b, q5 | 2 |  |
| **Part 1 Total** | | **10** |  |
| Part 2: Create a Basic Switch Configuration | Step 2 | 2 |  |
| Step 7b | 2 |  |
| Step 7c | 2 |  |
| Step 8 | 2 |  |
| **Part 2 Total** | | **8** |  |
| Part 3: Configure a MOTD Banner | Step 1, q1 | 2 |  |
| Step 1, q2 | 2 |  |
| **Part 3 Total** | | **4** |  |
| Part 4: Save Configuration Files to NVRAM | Step 2 | 2 |  |
| Step 3, q1 | 2 |  |
| Step 3, q2 | 2 |  |
| **Part 4 Total** | | **6** |  |
| **Packet Tracer Score** | | **72** |  |
| **Total Score** | | **100** |  |