**Packet Tracer - Configuring IPv6 Addressing**

**Addressing Table**

|  |  |  |  |
| --- | --- | --- | --- |
| **Device** | **Interface** | **IPv6 Address/Prefix** | **Default Gateway** |
| R1 | G0/0 | 2001:DB8:1:1::1/64 | N/A |
| G0/1 | 2001:DB8:1:2::1/64 | N/A |
| S0/0/0 | 2001:DB8:1:A001::2/64 | N/A |
| Link-local | FE80::1 | N/A |
| Sales | NIC | 2001:DB8:1:1::2/64 | FE80::1 |
| Billing | NIC | 2001:DB8:1:1::3/64 | FE80::1 |
| Accounting | NIC | 2001:DB8:1:1::4/64 | FE80::1 |
| Design | NIC | 2001:DB8:1:2::2/64 | FE80::1 |
| Engineering | NIC | 2001:DB8:1:2::3/64 | FE80::1 |
| CAD | NIC | 2001:DB8:1:2::4/64 | FE80::1 |

**Objectives**

**Part 1: Configure IPv6 Addressing on the Router**

**Part 2: Configure IPv6 Addressing on Servers**

**Part 3: Configure IPv6 Addressing on Clients**

**Part 4: Test and Verify Network Connectivity**

**Background**

In this activity, you will practice configuring IPv6 addresses on a router, servers, and clients. You will also practice verifying your IPv6 addressing implementation.

**Part 1:     Configure IPv6 Addressing on the Router**

**Step 1:     Enable the router to forward IPv6 packets.**

a.     Enter the ipv6 unicast-routing global configuration command. This command must be configured to enable the router to forward IPv6 packets. This command will be discussed in a later semester.

R1(config)# ipv6 unicast-routing

**Step 2:     Configure IPv6 addressing on GigabitEthernet0/0.**

a.     Click **R1** and then the **CLI**tab. Press **Enter**.

b.    Enter privileged EXEC mode.

c.     Enter the commands necessary to transition to interface configuration mode for GigabitEthernet0/0.

d.    Configure the IPv6 address with the following command:

R1(config-if)# **ipv6 address 2001:DB8:1:1::1/64**

e.     Configure the link-local IPv6 address with the following command:

R1(config-if)# **ipv6 address FE80::1 link-local**

f.     Activate the interface.

**Step 3:     Configure IPv6 addressing on GigabitEthernet0/1.**

a.     Enter the commands necessary to transition to interface configuration mode for GigabitEthernet0/1.

b.    Refer to the **Addressing Table** to obtain the correct IPv6 address.

c.     Configure the IPv6 address, the link-local address and activate the interface.

**Step 4:     Configure IPv6 addressing on Serial0/0/0.**

a.     Enter the commands necessary to transition to interface configuration mode for Serial0/0/0.

b.    Refer to the **Addressing Table** to obtain the correct IPv6 address.

c.     Configure the IPv6 address, the link-local and activate the interface.

**Part 2:     Configure IPv6 Addressing on the Servers**

**Step 1:     Configure IPv6 addressing on the Accounting Server.**

a.     Click **Accounting** and click the **Desktop**tab > **IP Configuration**.

b.    Set the **IPv6 Address** to **2001:DB8:1:1::4** with a prefix of **/64**.

c.     Set the **IPv6 Gateway** to the link-local address, **FE80::1**.

**Step 2:     Configure IPv6 addressing on the CAD Server.**

Repeat Steps 1a to 1c for the **CAD** server. Refer to the **Addressing Table**for the IPv6 address.

**Part 3:     Configure IPv6 Addressing on the Clients**

**Step 1:     Configure IPv6 addressing on the Sales and Billing Clients.**

a.     Click **Billing** and then select the **Desktop**tab followed by **IP Configuration**.

b.    Set the **IPv6 Address** to **2001:DB8:1:1::3** with a prefix of **/64**.

c.     Set the **IPv6 Gateway** to the link-local address, **FE80::1**.

d.    Repeat Steps 1a through 1c for **Sales**. Refer to the **Addressing Table**for the IPv6 address.

**Step 2:     Configure IPv6 Addressing on the Engineering and Design Clients.**

a.     Click **Engineering** and then select the **Desktop**tab followed by **IP Configuration**.

b.    Set the **IPv6 Address** to **2001:DB8:1:2::3**with a prefix of **/64**.

c.     Set the **IPv6 Gateway** to the link-local address, **FE80::1**.

d.    Repeat Steps 1a through 1c for **Design**. Refer to the **Addressing Table**for the IPv6 address.

**Part 4:     Test and Verify Network Connectivity**

**Step 1:     Open the server web pages from the clients.**

a.     Click **Sales** and click the **Desktop**tab. Close the **IP Configuration**window, if necessary.

b.    Click **Web Browser**. Enter **2001:DB8:1:1::4** in the URL box and click **Go**. The **Accounting** website should appear.

c.     Enter **2001:DB8:1:2::4** in the URL box and click **Go**. The **CAD** website should appear.

d.    Repeat steps 1a through 1d for the rest of the clients.

**Step 2:     Ping the ISP.**

a.     Open any client computer configuration window by clicking the icon.

b.    Click the **Desktop**tab > **Command Prompt**.

c.     Test connectivity to the ISP by entering the following command:

PC> **ping 2001:DB8:1:A001::1**

d.    Repeat the **ping** command with other clients until full connectivity is verified.